Devise a test to measure the current through a diode in a DC circuit.  The test results must record both the current through and the voltage across the diode; include a check for the reverse bias current up to 24V.

Your manager wants a diode that will allow equipment to receive positive from the power supply but protect from negative or reverse connection…

You have been told that a Zener diode can be used to regulate the voltage of a power supply unit – explain how the circuit you design will do that…

You have a customer who wants a thousand LEDs with current dropping resistors for Diwali – the LEDs are 0.02A maximum and the forward bias for the diode is 2.6V  (coloured LED). Design a circuit for connection to a PP3 battery.

[bookmark: _GoBack]You need an AC to DC converter in the region of 12V – the output must be DC with little ripple describe a suitable circuit for this…
